# Settings

##

You can specify the accuracy with which the position of the laser beam is indicated as "centred" on the reception area (54).

The current setting for the centre line indicator (l) can be seen in the indicator for reception accuracy.

1. To change the reception accuracy, press the button as many times as needed for the required setting to be shown on the display.

Each time you press the button, the relevant reception accuracy value appears briefly in the text display (n).

The setting for reception accuracy is saved when the tool is switched off.

##

The position of the laser beam on the reception area (54) can also be indicated by an audio signal.

The volume level can be changed or the audio signal switched off.

1. To change the volume level or switch off the audio signal, press the button until the required volume level is indicated on the display.

At a low volume, the audio signal indicator (p) appears on the display with one bar; at a high volume, the indicator appears with three bars. When the audio signal is switched off, the indicator goes out.

Independent of the audio signal setting, a short beep sounds at low volume level when the laser beam first makes contact with the reception area (54).

The setting for the audio signal is saved when the laser receiver is switched off.

##

Calling up the settings menu: Briefly press the button and the button simultaneously.

Changing a setting within a submenu: Press either the button or the button to switch between the settings. The last selected setting is automatically saved when exiting the menu.

Changing the submenu: Briefly press the button to go the next submenu.

Exiting the settings menu: Press and hold the button until the settings menu is closed. Alternatively, the settings menu is closed automatically about 10 seconds after the last button is pressed.

The following submenus are available:

- Unit of measurement of the relative height indicator: When calling up the unit of measurement menu, the currently selected unit of measurement is shown in the text display (n), while the available units of measurement are shown in the unit of measurement indicator (m) above it.
- LED direction indicators (LED): The 3 LED direction indicators (55), (57) and (56) can be adjusted with regard to their brightness or switched off. The LEDs light up in their selected setting.
- Display lighting (LIT): The display lighting can be switched on (green LED lights up) or switched off (red LED lights up).
- Memory function for last reception (MEM): The indicator for the direction in which the laser beam has left the reception area can be switched on (green LED lights up) or switched off (red LED lights up).
- LR 65 G: Centre functions (CF/CL): You can choose between CenterFind mode (CF) and CenterLock mode (CL). The current mode appears in the text display (n).

With the exception of the setting for the display lighting, all settings are saved when the laser receiver is switched off.

##

The displays (58) on the front and rear of the laser receiver can be illuminated. The display illumination function is switched on:

- When the laser receiver is switched on
- With each press of a button
- If the laser beam moves over the reception area (54).

The display illumination function automatically switches off:

- 30 s after each button press, if no laser beam reaches the reception area
- 2 min after the last button press and if the position of the laser beam in the reception area does not change.

The display lighting can be switched off in the settings menu.

The setting for display illumination is not saved when the laser receiver is switched off. After switching on the laser receiver, the display illumination is always switched on.