# Overview of control options for the functions

Function | GRL 600 CHV | GRL 650 CHVG | RC 6 | LR 60 | LR 65 G | Bosch Levelling Remote App
--- | --- | --- | --- | --- | --- | ---
Switching the GRL 600 CHV/GRL 650 CHVG on and off | ● | ● | − | − | − | −
Establish connection via Bluetooth®A) | ● | ● | ● | ● | ● | ●
Sleep mode | ● | ● | ● | − | − | ●
Switching on the keyboard lock | − | − | − | − | − | ●
Switching off the keyboard lock | ● | ● | − | − | − | ●
Rotation, line and point operation | ● | ● | ● | − | − | ●
Turning the line/point within the rotational plane | ● | ● | ● | − | − | ●
Turning the rotational plane when in the ‌vertical position | ● | ● | ● | − | − | ●
Automatic downwards plumb point function in the vertical position | − | − | ● | − | − | ●
Switching on/off the shock-warning function | ● | ● | − | − | − | ●
Adjusting the shock-warning function sensitivity | − | ● | − | − | − | ●
Slope operation | ● | ● | ● | − | − | ●
Changing Slope Protect (GRL 650 CHVG) | − | − | − | − | − | ●
Manual operation | ● | ● | − | − | − | ●
CenterFind mode | − | − | − | ● | ● | −
CenterLock mode | − | − | − | − | ● | −
Mask mode | − | − | − | − | − | ●
X-axis and Y-axis calibration (horizontal position)B) | ● | ● | − | ● | ● | ●
Z-axis calibration (vertical position) | ● | ● | − | − | − | ●

A)

  The function must be started on both the measuring tool and the remote control, laser receiver or smart phone at the same time.

B)

  The function must be started on both the measuring tool and the smartphone at the same time or on the laser receiver.