# Assignment of Functions

Function possible with LR 60 and | GRL 600 CHV | Rotary laser with red laser beam (600−800 nm)
--- | --- | ---
Battery charge indicator of the rotary laser | ● | −
Direction indicators for the position of the laser beam | ● | ●
Relative height indicator | ● | ●
CenterFind mode | ● | −

Function possible with LR 65 G and | GRL 650 CHVG | Rotary laser with green laser beam (500−570 nm)
--- | --- | ---
Battery charge indicator of the rotary laser | ● | −
Direction indicators for the position of the laser beam | ● | ●
Relative height indicator | ● | ●
CenterFind mode | ● | −
CenterLock mode | ● | −