# Technical data

Plunge router |  | GOF 20-12
--- | --- | ---
Article number |  | ‎3 601 F27 2..‎‎‎‎
Rated power input | W | 2000
No-load speed | min-1 | 10000–25000
Speed preselection |  | ●
Constant electronic control |  | ●
Connection for dust extraction |  | ●
Compatible collets | mm inches | 8–12 ¼–½
Router cage stroke | mm | 80
WeightA) | kg | 6.3
Protection class |  | / II

A)

  Without mains connection cable

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.