# Product features

The numbering of the product features refers to the diagram of the power tool on the graphics page.

(1) | Right handle (insulated gripping surface)
(2) | Spindle lock button
(3) | Chip protection
(4) | Wing bolt for parallel guide rods (2x)
(5) | Base plate
(6) | Guide plate
(7) | Holder for parallel guide rods
(8) | Step buffer
(9) | Wing bolt for depth stop adjustment
(10) | Slide with index mark
(11) | Left handle (insulated gripping surface)
(12) | Clamping lever for locking the routing depth
(13) | Scale for setting the routing depth
(14) | Depth stop
(15) | Scale for fine adjustment of the routing depth
(16) | Adjustment knob for fine adjustment of depth-of-cut (plunge base)
(17) | Speed preselection thumbwheel
(18) | Router bitA)
(19) | On/off switch
(20) | Lock-on button and unlock key for on/off switch
(21) | Open-ended spanner (17 mm, 24 mm)
(22) | Cap nut with collet
(23) | Dust extraction adapter (plunge base)
(24) | Knurled screw for dust extraction adapter (2x)
(25) | Extraction hose (dia. 35 mm)A)
(26) | Dust extraction adapter (non-plunge base)A)
(27) | Intermediate ring for extraction adapterA)
(28) | Parallel guide
(29) | Wing bolt for parallel guide coarse adjustment
(30) | Guide rod for parallel guide
(31) | Knob for parallel guide fine adjustment
(32) | Centring pin
(33) | Adjustable fence for parallel guide
(34) | SDS guide-bushing adapter
(35) | Fastening screw for guide-bushing adapter (2x)
(36) | Release lever for guide-bushing adapter
(37) | Guide bushing
(38) | Plunge base
(39) | Fastening screw for guide plate
(40) | Centring pinA)
(41) | Extraction hood for edge routing
(42) | Guide wheelA)

A)

  This accessory is not part of the standard scope of delivery.