# Operation

- Replace the cutting jaws (3) if the cutting edges are chipped or deformed (see figure E). Refer to the further instructions see Replacing the Cutting Jaws.

- The cutting jaws (3) are extremely sharp. You should therefore always keep your hands away from cutting edges and moving parts. Do not cut short workpiece parts where your hands could get close to the cutting jaws. There is a risk of serious injury or of limbs being severed.

- Make sure that cutting jaws (3) of the correct size are fitted to the power tool and that both cutting jaws are oriented in the correct position. Before you start cutting, check the thread size printed on the cutting jaws.

- Before pressing the release switch (14), insert the threaded rod such that its screw threads match those of the stationary cutting jaw. If the screw threads are not aligned correctly, this could cause a break in the cutting jaws and cause personal injury from fragments being flung out.

Attaching the Fall Protection System
Starting Operation
Working Advice