# Technical Data

Threaded rod cutters |  | GGC 18V-12
--- | --- | ---
Article number |  | ‎3 601 JM8 0..‎
Rated voltage | V= | 18
Cutting capacity
Soft steel |  | M 6 x 1 M 8 x 1.25 M 10 x 1.5 M 12 x 1.75
Stainless steel |  | M 6 x 1 M 8 x 1.25 M 10 x 1.5
Dimensions (L x W x H) | mm | 221 x 133 x 272
WeightA) | kg | 3.4
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationB) and during storage | °C | −20 … +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V…
Recommended chargers |  | GAL 18...

A)

  without battery (you can find the battery weights on www.bosch-professional.com)

B)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.