# Maintenance and Cleaning

- Before carrying out any work on the power tool (e.g. maintenance, tool change etc.), remove the battery from the power tool. There is risk of injury from unintentionally pressing the on/off switch.

- To ensure safe and efficient operation, always keep the power tool and the ventilation slots clean.

- Replace a damaged dust protection cap immediately. It is recommended that you have use an after-sales service for this.

- Clean the tool holder (2) after each use.