# Functions

## Turning the Line/Point in a Horizontal Position within the Rotational Plane (see figure A)

When the measuring tool is in a horizontal position, the laser line or the laser point can be positioned within the rotational plane of the laser. Rotation is possible by 360°.

For this, manually turn the rotation head (10) to the required position or use the remote control: Press the button for clockwise rotation (23) on the remote control to rotate clockwise, and the button for anticlockwise rotation (24) on the remote control to rotate anticlockwise. In rotational operation, pressing the buttons has no effect.

## Turning the Rotational Plane when in the ‌Vertical Position (see figure B)

When the measuring tool is in the vertical position, it is possible to rotate the laser point, laser line or rotational plane around the vertical axis for easy sighting out or parallel alignment in a range of ±8 %.

Press the button for clockwise rotation (23) on the remote control to rotate clockwise.

Press the button for anticlockwise rotation (24) on the remote control to rotate anticlockwise.