# Remote Control Power Supply

Using alkali-manganese batteries is recommended to operate the remote control.

To open the battery compartment cover (29), push the locking mechanism (28) in the direction of the arrow and remove the battery compartment cover. Insert the battery.

When inserting the batteries, ensure that the polarity is correct according to the illustration on the inside of the battery compartment.

- Remove the battery from the remote control when not using it for longer periods. The battery can corrode and self-discharge in the remote control during prolonged storage.