# Technical Data

Rotating platform | RM 3
--- | ---
Article number |
Operating temperature | –10 °C to +50 °C
Storage temperature | –20 °C to +70 °C
Max. altitude | 2000 m
Relative air humidity max. | 90 %
Pollution degree according to IEC 61010-1 | 2A)
Weight according to EPTA-Procedure 01:2014 | 0.46 kg
Protection rating | IP54 (dust and splash-proof)

A)

  Only non-conductive deposits occur, whereby occasional temporary conductivity caused by condensation is expected.

For clear identification of your rotating platform, see the serial number on the type plate.

Remote control | RC 2
--- | ---
Article number |
Working rangeA) | 20 m
Operating temperature | –10 °C to +50 °C
Storage temperature | –20 °C to +70 °C
Max. altitude | 2000 m
Relative air humidity max. | 90 %
Pollution degree according to IEC 61010-1 | 2B)
Batteries | 3 × 1.5 V LR3 (AAA)
Weight according to EPTA-Procedure 01:2014 | 0.05 kg

A)

  The working range may be reduced by unfavourable environmental conditions (e.g. direct sunlight).

B)

  Only non-conductive deposits occur, whereby occasional temporary conductivity caused by condensation is expected.

For clear identification of your remote control, see the serial number on the type plate.