# Technical Data

## Europe

Drill |  | GBM 1600 RE
--- | --- | ---
Article number |  | 3 601 AB0 0..
Rated power input | W | 850
No-load speed | min–1 | 630
Rated torque | Nm | 11
Spindle collar diameter | mm | 43
Max. drilling diameter
Steel | mm | 16
Wood | mm | 40
Aluminium | mm | 16
Chuck capacity | mm | 3–16
Clockwise/anticlockwise rotation |  | ●
Maximum mixer paddle diameter | mm | 160
WeightA) | kg | 3.0
Protection class |  | / II

A)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

The specifications apply to the specified rated voltages. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.