# Technical Data

Magnetic drill | GBM 50-2
--- | ---
Article number |  | ‎3 601 AB4 0..‎
Rated power input | W | 1200
No-load speed
First gear | min-1 | 50−250
Second gear | min-1 | 100−510
Laser type | nm | 635
| mW | < 1
Laser class |  | 2
C6 |  | 1
Divergence of laser line | mrad (full angle) | 0.5
Max. drilling diameter
Annular cutter | mm | 50
Twist drill bit | mm | 23
Screw tap |  | M16
Tool holder |  | MT2–DIN 228
Magnet retention force | kN | 14
Max. drill stroke | mm | 165
Magnetic base dimensions (width x depth x height) | mm | 200 x 98 x 38.5
WeightA) | kg | 14.7
Protection class |  | /I

A)

  Weight without mains connection cable and without mains plug

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.