# Symbols

The following symbols may be important for the operation of your power tool. Please take note of these symbols and their meaning. Correctly interpreting the symbols will help you to operate the power tool more effectively and safely.

Symbols and their meaning
| Do not direct the laser beam at persons or animals and do not stare into the direct or reflected laser beam yourself.
| Wear safety goggles.
| WARNING! If the beam of the overload indicator lights up close to the left symbol, the workload is very high. Reduce the workload or switch the motor off, otherwise the overload protection will be activated and the motor will be shut off automatically. If the beam of the overload indicator lights up close to the right symbol, the workload is optimal and there is no overload.
| WARNING! The tool must not be operated outside in wet weather.
| WARNING! Ensure that the safety strap is working properly before you use it. Never use a safety strap if it is damaged. Instead, replace it immediately.
| Persons with pacemakers or other medical implants must not use this power tool.
| Carrying metal parts or wearing watches is prohibited. The magnet generates a field that can impair the function of implants and medical devices.
| WARNING! When drilling into vertical or diagonal surfaces or overhead, the power tool must be secured with the safety strap.
| WARNING! Do not hold your hand underneath the application tool or the accessories when you are changing these.
| WARNING! Before drilling, ensure that the magnet strength is sufficient. The surface of the workpiece must be level, clean and sufficiently thick.