# Starting Operation

- Pay attention to the mains voltage. The voltage of the power source must match the voltage specified on the rating plate of the power tool.

- Products that are only sold in AUS and NZ: Use a residual current device (RCD) with a nominal residual current of 30 mA or less.

##

- Position and secure the power tool.
- To switch on the power tool, push the motor on/off switch (9) to position "I".

Note: The power tool can only be switched on once the magnet has already been activated.

##

- To switch off the power tool, push the motor on/off switch (9) to position "0".
- Wait until the power tool has come to a complete stop.
- Push the magnet on/off switch (20) downwards to switch off the magnet.

##

The restart protection feature prevents the power tool from uncontrolled starting after the power supply to it has been interrupted.

- To restart the power tool, push the motor on/off switch (9) to position "I".

Note: Once the power supply has been restored, press the RESET button on the residual current device (15). The magnet switches on automatically as soon as the indicator (16) on the residual current device (15) lights up red.

##

The power tool is equipped with an overload protection system. In normal conditions of use, the power tool cannot be overloaded. In the event of overloading, the power tool automatically shuts off the electronics. The magnet will remain active.

- To start the power tool again after this, press the motor on/off switch (9) into position "I".

Carry out the following steps before you continue working with the power tool:

- Eliminate any blockages that may be present. If the application tool jams, the anti-clockwise rotation function must not be used.
- Allow the power tool to run with no load for approx. one minute; afterwards, it will be ready for use again.

### Overload indicator

The overload indicator (6) indicates whether an overload has occurred when the power tool is switched on.

Overload indicator (6) | Overload
--- | ---
Green continuous light | No overload
Yellow continuous light | Heavy workload Reduce feed speed
Red flashing light | Very heavy workload Reduce feed speed or switch off motor, otherwise overload protection will be activated