# Technical Data

Mixer |  | GRW 18V-120
--- | --- | ---
Article number |  | ‎3 601 AC2 0..‎
Rated voltage | V= | 18
Soft start |  | ●
Speed preselection |  | ●
Constant electronic control |  | ●
KickBack Control |  | ●
No-load speedA) | min–1 | 0–600
Tool holder |  | M14
Maximum mixer paddle diameter | mm | 120
WeightB) | kg | 2.9
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Compatible rechargeable batteries |  | GBA 18V... ProCORE18V...
Recommended rechargeable batteries for maximum performance |  | ProCORE18V... ≥ 5.5 Ah
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery ProCORE18V 8.0Ah

B)

  without battery (you can find the battery weight on www.bosch-professional.com.)

C)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.