# Technical Data

Mixer |  | GRW 140
--- | --- | ---
Article number |  | ‎3 601 AC4 0..‎
Rated power input | W | 1400
Power output | W | 500
Mechanical gear selection |  | ●
Soft start |  | ●
Speed preselection |  | ●
Constant electronic control |  | ●
Restart protection |  | ●
No-load speed
First gear | min–1 | 200–480
Second gear | min–1 | 300–750
Rated torque
First gear | Nm | 10.2
Second gear | Nm | 6.7
Tool holder |  | M14
Maximum mixer paddle diameter | mm | 140
WeightA) | kg | 4.2
Protection class |  | / II

A)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.