# Work instructions for mixing

- Avoid splashing the material. Otherwise you could slip and lose control of the power tool.

- Avoid continuously operating the power tool at reduced speed. Otherwise the motor of the power tool could overheat.

Selection of the mixer basket is dependent on the mixing material that is to be mixed.

For mixing materials with low viscosity, e.g. emulsion paint, varnishes, adhesive, grouting compound or cement slurry, use a mixer basket with a left-hand spiral. The material is moved from the top downwards in a mixer basket with a left-hand spiral. The mixer basket is pushed upwards. Mixing materials with low viscosity are mixed in a way which minimises splattering.

For mixing materials with high viscosity, e.g. ready-mixed plaster, concrete, cement, screed, filler or epoxy resin, use a mixer basket with right-hand spiral. The material is moved from the bottom upwards in a mixer basket with a right-hand spiral. The mixer basket works its way into the mixture. Mixing materials with high viscosity are mixed thoroughly.

Move the power tool up and down when working. Clean the mixer basket after use.

- Store the power tool in a safe place. Ensure that it cannot fall over. The power tool may become damaged if this happens.