# Starting Operation

##

Open the top flap (10) and push the micro SD card (20) all the way into the slot (11). Close the top flap again.

##

To switch on the inspection camera, press the On/Off button (3). The start screen is shown in the display (9) for a short time.

Note: If the camera cable is not fitted when switching on, the display will show an error message.

To switch off the inspection camera, press the On/Off button (3) again.

If no button is pressed on the inspection camera, it switches off automatically after the set time has expired (k).

##

To brighten the camera image, you can switch on the light (15) in the camera head and regulate the brightness.

There are 4 settings for adjusting the brightness (0 %, 25 %, 50 %, 100 %).

To switch on the camera light (15) and increase the brightness, press the lighting/brightness button (7) repeatedly until the required brightness level has been reached.

- Do not look directly into the light (15) and do not direct the light onto other people. The light can blind your eyes.

To reduce brightness and switch off the camera light (15), press the lighting/brightness button (7) repeatedly until the required brightness level has been reached or the light has been switched off.

##

Briefly pressing the magnification button (2) magnifies the image in the display by a factor of 1.5 or 2.

##

The Up is Up™ button (5) rotates the image so that the "top" is shown at the top of the display.

Note: Limited function if mirror (25) is fitted and/or with a vertically aligned camera cable (13)

##

Switch between photo and video mode with the button for switching between photo and video mode (8). The currently selected recording mode (a) is displayed in the status bar (b).

Take a photo in the relevant mode or start and stop a video recording with the actuator for photo or video recordings or playing videos (6).

##

Pressing the (4) button assigns another function to the (8), (7), (5) and (4) buttons (according to the depiction in the display) (2nd level). Use these buttons according to the depiction in the display.

Briefly pressing the (4) button opens gallery mode. By pressing the (4) button you can see the image in full screen and by pressing the (6) button you can play a video.

Pressing the (4) button for a long time opens the mode settings. The following settings are possible:

- Colour rendition (red point)/black and white rendition (green point) (h)
- Brightness of display (i)
- Date/time (j)
- Auto off function: Length of inactivity of inspection camera after which it switches off (k)
- Lighting duration of the display (l)
- Memory space assignment/formatting of Micro-SD card (m)

##

The status bar (b) is shown on the display for approx. 2 seconds each time a button is pressed. It shows:

- The selected recording mode (a)
- Date and time
- The selected magnification (c)
- The selected brightness (i)
- The state of charge of the rechargeable battery/non-rechargeable batteries (e)

##

Transferring images and videos is only possible with an inserted Micro-SD card (20).

The inspection camera can be connected to a computer using a Micro-USB cable (19), to transfer images and videos.

Note: The USB port cannot be used with Apple products (e.g. MacBooks). Data transfer functions only via the Micro-SD card in this case.

A symbol in the display of the inspection camera shows that it is connected to a computer.

The inspection camera is displayed on the computer as an external drive.

The rechargeable battery of the inspection camera cannot be charged via the connection (12).

##

Open the top flap (10) and put the Micro-USB cable (19) into the connection (12) in the correct position.

After the data has been transferred, remove the Micro-USB cable and close the top flap again.