# Technical Data

Digital inspection camera |  | GIC 120 C
--- | --- | ---
Article number |  | ‎3 601 B41 2..‎‎‎‎
Rated voltage
With rechargeable battery | V= | 10.8/12
With non-rechargeable batteries | V= | 6
Non-rechargeable batteries (alkaline manganese) |  | 4 × 1.5 V LR6 (AA)
Relative air humidity | % | 5–95A)
Length of camera cable | m | 1.2
Smallest bend radius of camera cable | mm | 25
Camera head diameter | mm | 8.5
Display resolution |  | 320 × 240
Approx. operating time | h | 2B)/6C)
Weight according to ‌EPTA-Procedure 01:2014 | kg | 0.64
Dimensions (length × width × height) | mm | 217 × 90 × 49
Environmental conditions
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationD) | °C | –10 to +50
Permitted ambient temperature during storage without a rechargeable battery | °C | –20 to +70
Permitted ambient temperature during storage with a rechargeable battery | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 10,8V... GBA 12V...
Recommended chargers |  | GAL 12...

A)

  Free of condensation

B)

  With non-rechargeable batteries

C)

  With rechargeable battery at 100 % brightness of the light in the camera head

D)

  Limited performance at temperatures <0 °C