# Technical Data

Digital inspection camera |  | GIC 4-23 C | GIC 5-27 C
--- | --- | --- | ---
Article number |  | ‎3 601 B41 5K0‎‎‎‎ | ‎3 601 B41 4K0‎‎‎‎
Display size | " | 4.3 | 5
Display resolution | px | 800 × 480 | 1280 × 720
Resolution of camera/image filesA) | px | 1280 × 720 |
Camera resolution, photo and video files | px |  | 1280 × 720
Screenshot format |  | JPG | JPG
Video format |  | – | AVI
Video frame rate
without AutoUp function | fps | – | 20
with AutoUp function | fps | – | 7
Max. number of photos in internal memory |  | 30 | 30
Field of viewB) | ° | 75 | 75
Focus distance | mm | 30–80 | 30–80
Max. luminous intensity of the illumination light in the camera headC) | lx | 200 | 200
Max. immersion time for camera head/cable in diesel, engine oil, ethyl alcohol, petrol, AdBlue® or salt water (26.5% salt content) | min | 30 | 30
Power supply
Rechargeable battery (Li-ion) |  | 10.8 V/12 V | 10.8 V/12 V
Non-rechargeable batteries (alkaline manganese, with battery adapter) |  | 4 × 1.5 V LR6 (AA) | 4 × 1.5 V LR6 (AA)
Rechargeable batteries (NiMH, with battery adapter) |  | 4 × 1.2 V HR6 (AA) | 4 × 1.2 V HR6 (AA)
Backup power supply for saving the time
Coin cell |  | CR2450 (3 V, lithium battery) | CR2450 (3 V, lithium battery)
Battery life approx. | Years | 3 | 3
Operating time, approx.
With rechargeable battery (Li-ion)D) | h | 8E) | 6F)
With non-rechargeable batteries (alkaline manganese) | h | 3E) | 2F)
With rechargeable batteries (NiMH, 1.2 V) | h | 3.5E) | 3F)
Weight according to EPTA-Procedure 01:2014
With rechargeable battery (Li-ion) | kg | 0.73–0.94G) | 0.73–0.94G)
With non-rechargeable batteries (alkaline manganese) | kg | 0.68 | 0.68
Dimensions (length × width × height)D) | mm | 242 × 140 × 66 | 242 × 140 × 66
Camera head diameter | mm | 8.3 | 8.3
Length of camera cable | m | 1.5 | 1.5
Smallest bend radius of camera cable | mm | 25 | 25
Protection rating of handheld device (without rechargeable battery/battery adapter) |  | IP54 | IP54
Protection rating of camera head and camera cable |  | IP67 | IP67
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operation | °C | –10 to +50 | –10 to +50
Permitted ambient temperature during storage (without a rechargeable battery) | °C | –20 to +70 | –20 to +70
Recommended rechargeable batteries |  | GBA 10,8V… GBA 12V… | GBA 10,8V… GBA 12V…
Recommended chargers |  | GAL 12… GAX 18 … | GAL 12… GAX 18 …

A)

  Resolution 800 × 480, if the image is enlarged in the display or is displayed in black and white

B)

  Measured across the diagonal of the image

C)

  at 50 mm distance in a dark environment

D)

  with GBA 12V 2.0Ah

E)

  with camera display, with Up Indication function, average display brightness, illumination light with 50 % brightness

F)

  with camera display, with AutoUp function, average display brightness, illumination light with 50 % brightness

G)

  Depends on battery in use