# Main Menu

To access the <Main menu>, press the centre button (11).

## Navigating in the menu

- To scroll through a menu: Press the up (9) or down (12) buttons.
- To switch to a submenu: Press the centre button (11) or the right-hand button (13).
- To confirm a selected menu option: Press the centre button (11).
- To switch a function with a virtual switch on or off : Either press the centre button (11), the right-hand button (13) or the left-hand button (10). This will also save the setting.
- To return to the previous, higher-level menu: Briefly press the ON/OFF button (8).
- To exit the main menu and return to the camera display: Briefly press the ON/OFF button (8).

## Menu options

- <Up Indication> (GIC 4‑23 C): Switch the function on or off.
  When the Up Indication function is switched on, the arrow of the direction indicator (b), shows where "up" is in the image (see figure F).
  Note: The function is limited if a mirror (28) is fitted and/or with a vertically aligned camera cable (1).

- <AutoUp> (GIC 5‑27 C): Switch the function on or off.
  The AutoUp function rotates the image so that the "top" is shown at the top of the display (see figure G).
  Note: The function is limited if a mirror (28) is fitted and/or with a vertically aligned camera cable (1).

- <Gallery> (GIC 4‑23 C): This is where recorded photos can be accessed.
  You can select the required file based on its date using the down (12) or up (9) buttons.
  Press the right-hand button (13) or the centre button (11) to see a preview of the selected photo.
  To open the selected file, press the centre button (11).

- <Gallery> (GIC 5‑27 C): This is where recorded photos and videos can be accessed.
  You can select the required file based on its date using the down (12) or up (9) buttons.
  Press the right-hand button (13) or the centre button (11) to see a preview of the selected photo or video.
  To open the selected file, press the centre button (11).
  Note: If a micro-SD card (30) is inserted, only files saved on this micro-SD card are displayed. To open photos from the internal storage, you must first remove the micro-SD card (30).

- <Camera mode> (GIC 5‑27 C): Choose between <Photo> and <Video> for recordings.

- <Display brightness>: Set the required brightness for the display.

- <Color>: Switch between the colour view and black/white view of the display.

- <Device settings>

- <Date & time>: You can set the date and time for saving files and select the date and time format.
  Note: If the date and time can no longer be saved, the built-in coin cell is drained. Contact an authorised Bosch-after-sales service centre if this happens.
- <Language>: Select the language used in the display.
- <‎Switch off after …‎>: Choose the time interval after which the inspection camera will switch off automatically if no button is pressed.

- <Device info>: Here you will find device information, such as the installed software version and legal information.

- <Factory reset>: You can reset all of the menu options to factory settings. This also simultaneously, permanently delete all of the saved files.