# Technical Data

Heat gun | GHG 20‑60
--- | ---
Article number |  | ‎3 601 BA6 4..‎‎‎‎
Rated power input | W | 2000
Airflow | l/min l/min | 150–300 300–500
Temperature at the nozzle outletA) | °C | 50–630
Temperature measurement accuracy |  | ±10 %
Weight according to EPTA-Procedure 01:2014 | kg | 0.55
Protection class |  | /Ⅱ

A)

  At an ambient temperature of 20 °C

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.