# Technical Data

Heat gun | GHG 18V-50
--- | ---
Article number |  | ‎3 601 BA6 5..‎‎‎‎
Rated voltage | V= | 18
Max. airflow | l/min | 175
Temperature at the nozzle outletA) | °C | 300/500
Temperature measurement accuracy |  | ±10 %
Weight according to EPTA-Procedure 01:2014 | kg | 0.93–2.0B)
Dimensions (length × width × height) | mm | 183 × 77 × 209
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Compatible rechargeable batteries |  | GBA 18V… ProCORE18V…
Recommended rechargeable batteries |  | GBA 18V… ≥ 4.0 Ah ProCORE18V… ≥ 4.0 Ah
Recommended chargers |  | GAL 18… GAX 18… GAL 36…

A)

  At an ambient temperature of 20 °C

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.