# Technical Data

Random orbit sander |  | GEX 185‑LI
--- | --- | ---
Article number |  | ‎3 601 CA5 0..‎‎‎‎
Rated voltage | V | 18
Orbital stroke rate preselection |  | ●
No-load speed n₀A) | min−1 | 6,000–10,000
No-load orbital stroke rateA) | min−1 | 12,000–20,000
Orbit diameter | mm | 2.5
Sanding pad diameter | mm | 125
WeightB) | kg | 1.3–2.3
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | −15 to +50
Recommended rechargeable batteries |  | GBA 18V… ProCORE18V…
Recommended battery chargers |  | GAL 18… GAX 18… GAL 36…

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 4.0Ah

B)

  Depending on battery in use

C)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.