# Changing the Sanding Pad (see figure B)

Note: Replace damaged sanding pads (5) immediately.

Pull off the sanding sheet. Unscrew the 4 screws (9) completely (using a T20 screwdriver) and remove the sanding pad (5). Attach the new sanding pad (5) and retighten the screws.

Note: When attaching the sanding pad, make sure that the teeth of the catch mate with the recesses in the sanding pad.

Note: Damaged sanding pad holders (10) must only be replaced by an after-sales service centre authorised to work with Bosch power tools.