# Technical Data

Angle grinder |  | GWS 12-125 P | GWS 12-125 S
--- | --- | --- | ---
Article number |  | ‎3 601 CA6 2..‎ | ‎3 601 CA6 0..‎
Rated power input | W | 1200 | 1200
Power output | W | 630 | 630
Rated no-load speedA) | min–1 | 11000 | 11000
Speed adjustment range | min–1 | – | 2800–11000
Max. grinding disc diameter/rubber sanding pad diameter | mm | 125 | 125
Grinding spindle thread |  | M 14 | M 14
Max. thread length of grinding spindle | mm | 22 | 22
Restart protection |  | ● | ●
Soft start |  | ● | ●
Constant electronic control |  | ● | ●
KickBack Control |  | ● | ●
Speed preselection |  | – | ●
WeightB) | kg | 2.1−2.4 | 2.0−2.4
Protection class |  | / II | / II

A)

  Rated no-load speed for the selection of appropriate application tools in accordance with EN IEC 62841-2-3. The actual no-load speed is lower for safety reasons and according to production tolerances.

B)

  Depends on protective guard ((8), (7), (9)) and auxiliary handle ((5), (4)) in use

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.