# Rotating the machine head (see figure E)

- Pull the plug out of the socket before carrying out any work on the power tool.

The machine head can be rotated in 90° increments. In this way, the on/off switch can be brought into a more favourable handling position for particular applications, e.g. for left-handed tool users.

Completely unscrew the four screws (➊). Rotate the machine head carefully, without removing it from the housing, into the new position (➋). Screw in and retighten the four screws (➌).