# Technical Data

Grinder |  | GWG 12V-50 S
--- | --- | ---
Article number |  | ‎3 601 CA7 0..‎
Rated voltage | V= | 12
max. speed nA) | min–1 | 16000
Speed adjustment range n1 | min–1 | 5000–15000
Max. collet diameter | mm | 8
Spanner flat on the
clamping nut | mm | 17
Max. grinding tool diameter | mm | 50
Speed preselection |  | ●
Constant electronic control |  | ●
Weight according to EPTA-Procedure 01:2014B) | kg | 0.71–0.91
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) | °C | –15 to +50
Permitted ambient temperature during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 12V...
Recommended chargers |  | GAL 12... GAX 18...

A)

  Measured at 20–25 °C with rechargeable battery GBA 12V 3.0Ah and depending on the battery's state of charge as well as the power tool's operating temperature

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.