# Noise/Vibration Information

Noise emission values determined according to EN 60745-2-23.

Typically, the A-weighted sound pressure level of the power tool is less than 70 dB(A). The noise level when working can exceed the volume stated. Wear hearing protection!

Total vibration values ah (triax vector sum) and uncertainty K determined according to EN 60745-2-23:

Surface grinding (roughing with grinding tool diameter of 25 mm):
ah < 2.5 m/s2, K = 1,5 m/s2

Surface grinding (roughing with grinding tool diameter of 50 mm):
ah = 13.2 m/s2, K = 1,5 m/s2

The vibration level given in these instructions has been measured in accordance with a standardised measuring procedure and may be used to compare power tools. It can also be used for a preliminary estimation of exposure to vibration.

The stated vibration level applies to the main applications of the power tool. However, if the power tool is used for different applications, with different application tools or poorly maintained, the vibration level may differ. This can significantly increase the exposure to vibration over the total working period.

To estimate the exposure to vibration accurately, the times when the tool is switched off or when it is running but not actually being used should also be taken into account. This can significantly reduce the exposure to vibration over the total working period.

Implement additional safety measures to protect the operator from the effects of vibration, such as servicing the power tool and application tools, keeping the hands warm, and organising workflows correctly.