# Technical Data

Cordless worklight |  | GLI VariLED
--- | --- | ---
Article number |  | ‎3 601 D43 4..‎ ‎
Rated voltage | V= | 18
Lighting duration, approx. | min/Ah | 190
Total luminous flux, max. | lm | 420
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationA) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V...
Recommended chargers |  | GAL 18... GAX 18... GAL 36...

A)

  Limited performance at temperatures < 0 °C

The colour rendition of illuminated objects can be distorted.