# Starting Operation

## Inserting the battery

Insert the charged battery (4) into lamp head (3) until it can be felt to engage and faces flush against the lamp head.

## Setting up

Place the cordless worklight on a stable, level surface. Make sure it is secure.

## Switching On and Off

To switch on the cordless worklight, press the on/off switch (2).

To switch off the cordless worklight, press the on/off switch (2) again.

## Temperature Dependent Overload Protection

If the permissible heat sink temperature of 60 °C is exceeded, the cordless worklight flashes 3 times and switches off. Let the cordless worklight cool down and then switch the cordless worklight back on.

## Battery charge indicator

The green LEDs on the battery charge indicator indicate the state of charge of the battery. For safety reasons, it is only possible to check the state of charge when the power tool is not in operation.

Press the button for the battery charge indicator or to show the state of charge. This is also possible when the battery is removed.

If no LED lights up after pressing the button for the battery charge indicator, then the battery is defective and must be replaced.

### Battery model GBA 18V...

×

LEDs | Capacity
--- | ---
3× continuous green light | 60−100 %
2× continuous green light | 30−60 %
1× continuous green light | 5−30 %
1× flashing green light | 0−5 %

### Battery model ProCORE18V...

×

LEDs | Capacity
--- | ---
5× continuous green light | 80−100 %
4× continuous green light | 60−80 %
3× continuous green light | 40−60 %
2× continuous green light | 20−40 %
1× continuous green light | 5−20 %
1× flashing green light | 0−5 %