# Technical Data

Cordless worklight |  | GLI 18V-1900
--- | --- | ---
Article number |  | ‎‎3 601 D46 4..‎‎‎‎‎‎‎‎
Rated voltage | V= | 18
Max. rated power input | W | 21
Lighting duration, approx. | min/Ah | 50
Total luminous flux, max. | lm | 1900
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationA) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V...
Recommended chargers |  | GAL 18... GAX 18... GAL 36...
Protection class |  | /III

A)

  Limited performance at temperatures < 0 °C

The colour rendition of illuminated objects can be distorted.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.