# Starting Operation

##

Carefully fold out the stand (5) and place the cordless worklight on the floor. Make sure it is secure.

##

You can use the tripod mount (7) to screw the cordless worklight onto a tripod.

Attach the cordless worklight firmly to the tripod. Ensure that the cordless worklight cannot come loose and/or fall over.

Ensure that the tripod has a firm footing.

##

The lamp head (4) is attached to the carrying handle (8). The lamp head can be set to five different positions using the carrying handle.

##

To switch on the cordless worklight, press the on/off switch (1).

To switch off the cordless worklight, press the on/off switch (1) again.

##

Press the on/off switch (1) briefly to switch on the cordless worklight with maximum brightness. To adjust the brightness in two stages, hold down the on/off switch (1) until the required brightness is reached.

##

If the permissible operating temperature is exceeded, the cordless worklight switches off. Let the cordless worklight cool down and then switch the cordless worklight back on.