# Technical Data

Cordless worklight |  | GLI 18V-2200 C
--- | --- | ---
Article number |  | ‎‎3 601 D46 5..‎‎‎‎‎‎‎‎
Rated voltage | V= | 18
Max. rated power input | W | 23
Lighting durationA), approx. | min/Ah | 44
Total luminous flux, max. | lm | 2200
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationB) and during storage | °C | –20 to +50
Coin cell | V type | 3 CR 2032
Recommended rechargeable batteries |  | GBA 18V... ProCORE18V... (max. 8.0 Ah)
Recommended chargers |  | GAL 18... GAX 18... GAL 36...
Protection class |  | /III
Protection ratingC) |  | IP64
Data transfer
Bluetooth®D) |  | Bluetooth® 4.1 (Low Energy)
Signal rangeE) | m | 15
Operating frequency range | MHz | 2402–2480
Max. transmission power | mW | < 2

A)

  At maximum brightness incl. remaining operating time in dimmed mode

B)

  Limited performance at temperatures < 0 °C

C)

  Applies only when battery cover is closed and locked

D)

  The mobile devices must be compatible with Bluetooth® Low Energy devices (version 4.1) and support the Generic Access Profile (GAP).

E)

  The signal range may vary greatly depending on external conditions, including the receiving device used. The Bluetooth® range may be significantly weaker inside closed rooms and through metallic barriers (e.g. walls, shelving units, cases, etc.).

The colour rendition of illuminated objects can be distorted.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.

System requirements
Mobile device (tablet, smartphone)A) | Android, iOS

A)

  Minimum system requirements can be found in the app store for your mobile device (e.g. Google Play Store or Apple App Store).