# Start-up

##

Carefully fold out the stand (5) and place the cordless worklight on the floor. Make sure it is secure.

##

You can use the tripod mount (7) to screw the cordless worklight onto a tripod.

Tighten the 5/8" screw. Ensure that the tripod has a firm footing.

##

The lamp head (4) is attached to the carrying handle (8). The lamp head can be set to five different positions using the carrying handle.

##

To start up the cordless worklight, press the on/off switch (1).

To switch off the cordless worklight, press the on/off switch (1) again.

##

Press the on/off switch (1) briefly to switch on the cordless worklight with maximum brightness. To adjust the brightness in two stages, hold down the on/off switch (1) until the required brightness is reached.

##

When the permitted operating temperature is exceeded, the cordless worklight initially reduces the brightness before switching itself off if required for protection. Let the cordless worklight cool down and then switch the cordless worklight back on.

##

- Make sure that the battery compartment (12) is not damaged when removing the coin cell.

- Make sure that the positive pole of the coin cell faces upwards.

A warning will be displayed in the app before the coin cell (11) is fully used up.

To change the coin cell (11), unlock the locking mechanism of the battery cover (2) and fold back the battery cover (3).

Unscrew the screw of the battery compartment cover (9) and remove the battery compartment cover (10).

Remove the empty coin cell and insert a new coin cell.

Reattach the battery compartment cover with the screw.