# Putting the Coin Cell into Operation (see figure A)

Remove the separating film between the coin cell (11) and the coin cell contact when using the tool for the first time.

The cordless worklight is fitted with a coin cell so that it can be detected by the mobile device even if no battery pack (14) is inserted.

Unlock the locking mechanism of the battery cover (2) and fold back the battery cover (3).

Unscrew the screw of the battery compartment cover (9) and remove the battery compartment cover (10).

Remove the film from the coin cell contact and reattach the battery compartment cover with the screw.