# Starting Operation

##

To switch on the cordless worklight, press the on/off switch (9).

To switch off the cordless worklight, press the on/off switch (9) again.

##

Press the on/off switch (9) briefly to switch on the cordless worklight with maximum brightness. To adjust the brightness in two stages, hold down the on/off switch (9) until the required brightness is reached.

##

If the permissible operating temperature is exceeded, the cordless worklight switches off. Let the cordless worklight cool down and then switch the cordless worklight back on.