# Practical Advice

Shortly before the cordless worklight switches off because of an empty battery, it will flash three times and shine with reduced brightness.

##

The lamp head (1) can be swivelled up to 200° to suit the application.

Examples of applications are:

- Room lighting
- Glare-free workplace lighting
- Floor lighting

Note: For an incline of more than 90°, the cordless worklight must be fastened in place.

##

You can use the utility hook (7) to attach the cordless worklight to an object.

##

You can use the snap hook (4) to attach the cordless worklight, e.g. to a rope or a belt.

##

You can use the magnets (6) to attach the cordless worklight to magnetic materials.

- Keep your fingers away from the rear side of the stand when attaching the cordless worklight to surfaces. The strong pulling force of the magnets may trap your fingers.

When attaching the cordless worklight, take care not to leave scratches on delicate surfaces.

##

You can use the tripod mount (8) to screw the cordless worklight onto a 1/4" tripod.

Tighten the cordless worklight using the locking screw of the tripod. Ensure that the tripod has a firm footing.