# Technical Data

Cordless worklight | GLI 12V-330
--- | ---
Article number |  | ‎‎3 601 DA0 0..‎‎‎‎‎‎‎‎
Rated voltage | V= | 12
Max. rated power input | W | 3.6
Lighting duration, approx. | min/Ah | 180
Luminous flux | lm | 330
Recommended ambient temperature during charging | °C | 0 … +35
Permitted ambient temperature during operationA) and during storage | °C | –20 … +40
Recommended rechargeable batteries |  | GBA 12V…
Recommended battery chargers |  | GAL 12… GAX 18…
Protection class |  | /III

A)

  Limited performance at temperatures < 0 °C

The colour rendition of illuminated objects can be distorted.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.