# Battery Charge Indicator

When the rechargeable battery is inserted, you can see the state of charge of the battery (26) in the display. When the rechargeable battery is removed, you can see this on the battery itself.

##

The battery charge indicator (b) will appear in the display as soon as a rechargeable battery with sufficient voltage is inserted and the radio is not connected to the mains supply.

Display | Capacity
--- | ---
| 80−100 %
| 60−80 %
| 40−60 %
| 20−40 %
| 5−20 %
| 0−5 %

##

If the rechargeable battery is removed from the radio, its state of charge may be indicated by the green LEDs of the battery charge indicator on the rechargeable battery.

Press the button for the battery charge indicator or to show the state of charge.

If no LED lights up after pressing the button for the battery charge indicator, then the battery is defective and must be replaced.

### Battery model GBA 18V...

LEDs | Capacity
--- | ---
3× continuous green light | 60−100 %
2× continuous green light | 30−60 %
1× continuous green light | 5−30 %
1× flashing green light | 0−5 %

### Battery model ProCORE18V...

LEDs | Capacity
--- | ---
5× continuous green light | 80−100 %
4× continuous green light | 60−80 %
3× continuous green light | 40−60 %
2× continuous green light | 20−40 %
1× continuous green light | 5−20 %
1× flashing green light | 0−5 %