# Technical data

Nibbler |  | GNA 18V-16 E
--- | --- | ---
Article number |  | ‎3 601 E29 6..‎‎‎‎
Rated voltage | V= | 18
No-load stroke rate n₀ | min−1 | 1400A)
Max. steel sheet cutting capacityB) | mm | 1.6
Cutting width | mm | 5
Smallest curve radius | mm | 40
WeightC) | kg | 2.1−3.1
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationD) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V… ProCORE18V…
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 4.0Ah and depending on the battery's state of charge as well as the power tool's operating temperature

B)

  with reference to steel sheet of up to 400 N/mm2

C)

  Depends on battery in use

D)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.