# Starting Operation

##

To switch on the power tool, slide the on/off switch (3) forwards so that I appears on the switch.

To switch off the power tool, slide the on/off switch (3) backwards so that 0 appears on the switch.

##

The restart protection feature prevents the power tool from uncontrolled starting after the power supply to it has been interrupted.

To restart the tool, set the on/off switch (3) to the off position and then switch the power tool on again.

##

The electronic soft start limits the torque when the power tool is switched on and increases the service life of the motor.

##

To change the cutting direction, the die holder (7) can be turned to three positions, each offset by 90°. Cutting towards the rear (towards the housing of the machine) is not possible.

To turn the die holder (7), loosen the die holder screw (4) until the die holder can be turned. Turn it 90° to the right or the left in relation to the longitudinal axle of the power tool.

Make sure that the screw (4) engages in the drill hole of the die holder (7). Tighten the screw.