# Technical data

Planer |  | GHO 185-LI
--- | --- | ---
Article number |  | ‎3 601 EB5 0..‎
Rated voltage | V | 18
No-load speedA) | min–1 | 14,000
Cutting depth | mm | 0–2.6
Rebate depth | mm | 0–9
Max. planing width | mm | 82
Weight according to EPTA-Procedure 01:2014B) | kg | 2.6–3.7
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V… ProCORE18V…
Recommended chargers |  | GAL 18… GAX 18… GAL 36…

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 4.0Ah.

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C

Values can vary depending upon the product and are subject to application and environmental conditions. For further information www.bosch-professional.com/wac.