# Setting the routing depth

- The routing depth must only be set while the power tool is switched off.

- Place the power tool with a fitted router bit onto the workpiece you want to machine.
- Reopen the wing bolt (12) on the routing base (2) in order to set the required routing depth based on the scale for setting routing depth (15) either by hand or with the knurled screw (6).
- Close the wing bolt (12) on the routing base (2).
- Check the routing depth you have set by carrying out a practical test and correct it if required.