# Technical Data

Circular Saw |  | GKS 140
--- | --- | ---
Article number |  | ‎3 601 FB3 0..‎
Rated power input | W | 1400
Rated no-load speed | min–1 | 6200
Max. cutting depth with 184 mm saw blade diameter
At a 0° mitre/bevel angle | mm | 64
At a 45° mitre/bevel angle | mm | 45
Spindle lock |  | ●
Base plate dimensions | mm | 290 x 150
Max./min. saw blade diameter | mm | 184
Max. base blade thickness | mm | 2.0
Locating bore | mm | 20
WeightA) | kg | 3.7
Protection class |  | / II

A)

  Weight without mains connection cable and without mains plug

The specifications apply to a rated voltage [U] of 230 V. These specifications may vary at different voltages and in country-specific models.

Turn-on transients cause brief drops in voltage. Interference with other tools may occur in the event of unfavourable conditions in the electricity supply. Malfunctions are not to be expected for system impedances below 1.539 ohm.

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.