# Start-up

- Pay attention to the mains voltage. The voltage of the power source must match the voltage specified on the rating plate of the power tool.

- Products that are only sold in AUS and NZ: Use a residual current device (RCD) with a nominal residual current of 30 mA or less.

## Switching on/off

- Make sure that you are able to press the On/Off switch without releasing the handle.

To start the power tool, first press the lock-off switch (2), then press and hold the on/off switch (1).

To switch off the power tool, release the on/off switch (1).

Note: For safety reasons, the on/off switch (1) cannot be locked; it must remain pressed during the entire operation.