# Technical data

Hand-held circular saw |  | GKS 18V-57-2 GX
--- | --- | ---
Article number |  | ‎3 601 FC1 0..‎
Rated voltage | V | 18
Rated no-load speedA) | min–1 | 5000
Max. cutting depth
at a 0° mitre/bevel angle | mm | 57
at a 45° mitre/bevel angle | mm | 42
Spindle lock |  | ●
Base plate dimensions | mm | 164 x 305
Saw blade diameter | mm | 165
Max. base blade thickness | mm | 1.8
Min. base blade thickness | mm | 0,9
Locating bore | mm | 20
WeightB) | kg | 4.7
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ≥ 2,0 Ah ProCORE18V... ≥ 4,0 Ah
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 5.5Ah

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.