# Technical data

Hand-held circular saw |  | GKS 185-LI
--- | --- | ---
Article number |  | ‎3 601 FC1 2..‎
Rated voltage | V | 18
No-load speedA) | min-1 | 5000
Max. cutting depth
at a 0° mitre/bevel angle | mm | 57
at a 45° mitre/bevel angle | mm | 41
Spindle lock |  | ●
Base plate dimensions | mm | 134 x 280
Saw blade diameter | mm | 165
Max. base blade thickness | mm | 1,8
Min. base blade thickness | mm | 0,9
Locating bore | mm | 20
Weight according to EPTA-Procedure 01:2014B) | kg | 3,2–4,3
Recommended ambient temperature during charging | °C | 0 to +35
Permitted ambient temperature during operationC) and during storage | °C | –20 to +50
Recommended rechargeable batteries |  | GBA 18V... ≥ 4,0 Ah ProCORE18V... ≥ 4,0 Ah
Recommended chargers |  | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery GBA 18V 5.0Ah.

B)

  Depends on battery in use

C)

  Limited performance at temperatures < 0 °C