# Start-up

##

- Make sure that you are able to press the On/Off switch without releasing the handle.

To start the power tool, first press the lock-off switch (2), then press and hold the on/off switch (1).

To switch off the power tool, release the on/off switch (1).

Note: For safety reasons, the on/off switch (1) cannot be locked; it must remain pressed during the entire operation.

##

The lamp (10) lights up when the on/off switch (1) is lightly or fully pressed, meaning that the work area is illuminated in poor lighting conditions.

##

An integrated run-out brake shortens the time the saw blade keeps running for after the power tool has been switched off.

##

The lithium-ion battery is protected against deep discharge by the Electronic Cell Protection (ECP). When the battery is discharged, the power tool is switched off by means of a protective circuit: The application tool no longer rotates.